

KIM Clone Quick Set-Up Guide

www.corshamtech.com

These are minimal instructions to get your KIM Clone board set up and running in the default KIM-1 mode:

1. Set the POWER switch to OFF.
2. Set SW3/VECTORS to KIM. This is located along the left edge of the board about half way up.
3. Set SW1/SST to OFF. This is located to the right of SW3.
4. Set SW2 to KBD. This switch is located above the seven segment LEDs.
5. Plug in the power supply to the nearest output.
6. Plug in the power cable to the 8 VDC jack on left side of the board.
7. Set the POWER switch to ON. The POWER LED near the POWER switch should light up.
8. Press the red RS (reset) button.

The LEDs should now be lit and your KIM Clone is ready to use! Please find more documentation on the included USB thumb drive.